April 5, 2017

Question & Answer 3

 Bid R634413

 Water Treatment Program

**Question 1**

Section 11.0   11.3   Treatment level for hot loops should be 400-600ppm can we run higher than that?

**Answer**

(If 400 – 600 PPM is the industry standard acceptable range then that is what we would ask to achieve)