**Q&A #1**

**RFP #R597661**

**Audio/Visual Services**

1. Question: On Page 11, beneath the heading teleprompter system, it reads “there will be a LED screen suspended . . . “ Does that mean there will be a screen already in place, or does the vendor supply the screen, processing electronics, rigging and power? If so, what are the specifics regarding the screen, i.e. the pixel pitch?

Answer: The vendor will provide a 20’ x 60’ LED screen with a preferred pixel pitch no greater than 6.0 and a brightness of no lower than 2,000 nits.